WHELEN M9 EZ SCENE LIGHT

(QUANTITY) Whelen M9 EZ Scene lights shall be supplied and mounted on the apparatus. The lights shall be provided with a (chrome or black) flange. The dimensions of the light are 10.35” x 6.28” H. 

LOCATIONS:

The lights shall be mounted on the apparatus in the following locations:
•	(QTY) on Left Side
•	(QTY) on Right Side
•	(QTY) on Rear

ACTIVATIONS: 
•	Detail Switched Activations: 
o	Cab Driverside
o	Cab Officerside
o	Pump Panel
o	Rear Body
•	Detail Activation Type:
o	Switch
o	Vista Screen
•	Detail Automatic Activations: 
o	Side Lights to activate on respective side when cab door is opened
o	Rear Lights to activate when unit is placed in reverse